Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-12-86
P. 64

    UF3V12E0.book  Page 58  Wednesday, June 3, 2020  2:38 PM

                            Equipment operation

                            To close the bow storage compartment:
                                                                    Glove compartment:
                            Push the rear of the hood down to securely  Capacity:
                            lock it in place.                           17.0 L (4.5 US gal, 3.7 Imp.gal)
                                                                      Load limit:
                                                                        1.0 kg (2 lb)

                                                                  To close the glove compartment:
                                                                  Lower the lid, and then hook the glove com-
                                                                  partment latch.

                            EJU45080
                            Glove compartment
                            The glove compartment is located in front of
                            the seat.
                            To open the glove compartment:
                            Unhook the glove compartment latch,  and
                            then lift up the lid.                 To drain water from the glove compartment:
                                                                  (1) Remove the drain plugs on the bottom of
                                                                     the glove compartment to drain the wa-
                                                                     ter.

                                                         1                              1

                              1 Glove compartment latch

                                                                   1 Drain plug
                                                                  (2) Securely install the drain plugs  in their
                                                                     original positions.
                                                        1
                                                                  EJU45220
                                                                  Stern storage compartment
                                                                  The stern storage compartment is located in
                                                                  front of the boarding platform.

                              1 Glove compartment

                            58

| 59 60 61 62 63 64 65 66 67 68 69 |