Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-12-86
P. 49

    UF3V12E0.book  Page 43  Wednesday, June 3, 2020  2:38 PM

                                                                      Watercraft operation

                                and the acceleration setting under “Ac-  To unlock the drive control mode screen:
                                cel.”                             (1) Release the throttle lever and let the en-
                                                                     gine speed return to idle.
                                        1          2
                                                                  (2) Tap the drive control mode indicator on
                                     Speed      Accel.               the multifunction information center.
                                     45 MPH      Slow             (3) The PIN entry screen will be displayed.
                                     45 MPH
                                     35 MPH
                                     35 MPH     Normal               Flick up or down to set each digit of the
                                     55 MPH
                                     55 MPH      Slow                4-digit PIN, and then tap the “Enter” but-
                                                                     ton.
                                            Save
                                                                  (4) Tap the “Lock” button.
                                                                  (5) Tap the “OFF” button.
                                                                  (6) Tap the “Save” button to complete the
                              1 Maximum watercraft speed setting
                                                                     setting and return to the “Drive Control”
                              2 Acceleration setting
                                                                     screen.
                            (4) Tap the “Save” button to complete the  EJU45021
                                                                  Cruise assist
                                settings and return to the previous dis-
                                                                  The cruise assist is a function for maintaining
                                play.
                                                                  a desired engine speed within a fixed range
                            To lock the drive control mode screen:
                                                                  while operating the watercraft. Once the
                            (1) Release the throttle lever and let the en-
                                                                  cruise assist is  activated, the  set  engine
                                gine speed return to idle.
                                                                  speed can be increased or decreased. How-
                            (2) Tap the drive control mode indicator on
                                                                  ever, the adjustment is limited to a maximum
                                the multifunction information center.
                                                                  of five increments above or below the initial
                            (3) Tap the “Lock” button.
                                                                  cruise assist setting.
                            (4) The PIN entry screen will be displayed.
                                Flick up or down to set each digit of the  TIP:
                                4-digit PIN, and then tap the “Enter” but-  The cruise assist can only be set between en-
                                ton.                              gine speeds of approximately 3000 r/min and
                            (5) Tap the “ON” button.              approximately 7000 r/min.
                                    Drive Control Lock
                                      ON          OFF

                                            Save

                            (6) Tap the “Save” button to complete the
                                setting and return to the “Drive Control”
                                screen.

                                                                                                   43

| 44 45 46 47 48 49 50 51 52 53 54 |