Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-12-86
P. 63

    UF3V12E0.book  Page 57  Wednesday, June 3, 2020  2:38 PM

                                                                     Equipment operation

                            could fall, which could result in severe in-  jects that must be kept dry, put them in a wa-
                            jury. [EWJ01511]                      terproof bag.
                                                                  Make sure  that the storage  compartments
                                                                  are closed securely before operating the wa-
                                                                  tercraft.
                                    1
                                                                  EJU45250
                                                                  Bow storage compartment
                                                                  The bow storage compartment is located un-
                                                                  der the hood.
                                                                  To open the bow storage compartment:
                                                                  Pull the hood latch rearward, and then lift up
                                                                  the rear of the hood.
                              1 Cleat
                                                                                           1
                            EJU34894
                            Pull-up cleats (FX CRUISER HO)
                            The pull-up cleats are used to attach a rope
                            to the watercraft when mooring it.
                            To use a pull-up cleat, pull it up. The pull-up
                            cleat returns automatically to its original posi-
                            tion when released. WARNING! Do not use
                            the pull-up cleats to lift the watercraft. The
                            pull-up cleats are not designed to support
                                                                   1 Hood latch
                            the watercraft’s weight. If the pull-up
                            cleats break, the watercraft could fall,
                            which could result in severe injury. [EWJ00822]

                                                           1
                                                                                1

                                                                   1 Bow storage compartment
                                                                    Bow storage compartment:
                                                                      Capacity:
                              1 Pull-up cleat
                                                                        130.0 L (34.3 US gal, 28.6 Imp.gal)
                            EJU35148                                  Load limit:
                            Storage compartments                        5.0 kg (11 lb)
                            This watercraft is equipped with the following
                            storage compartments.
                            Only the securely closed watertight storage
                            compartment is waterproof. If you carry ob-

                                                                                                   57

| 58 59 60 61 62 63 64 65 66 67 68 |