Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-86
P. 69

    UF3V12E0.book  Page 63  Wednesday, June 3, 2020  2:38 PM

                                             Operation and handling requirements

                                                                     Do not  leave the watercraft with  a full
                              Fuel tank capacity:
                                70 L (18.5 US gal, 15.4 Imp.gal)     tank in direct sunlight.

                                                                                          1
                                                                                            2

                                                                   1 Top of the fuel tank
                                                                   2 Approximately 50 mm (2 in) from top of the
                            (6) Stop filling  when the  fuel level reaches
                                                                     fuel tank
                                approximately 50 mm (2 in) from the top
                                of the fuel tank. Do not overfill the fuel                  1
                                tank. Because fuel expands when it                               2
                                heats up, heat from the engine or the sun
                                can cause fuel to spill out of the fuel tank.

                                                                   1 Top of the fuel tank
                                                                   2 Approximately 50 mm (2 in) from top of the
                                                                     fuel tank
                                                                  (7) Wipe up any spilled fuel immediately with
                                                                     a dry cloth.
                                                                  (8) Securely install the fuel filler cap by tight-
                                                                     ening it until it clicks.
                                                                  (9) Securely install the seats in their original
                                                                     positions.

                                                                                                   63

| 64 65 66 67 68 69 70 71 72 73 74 |