Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 83 - LIT-18626-12-86
P. 83

    UF3V12E0.book  Page 77  Wednesday, June 3, 2020  2:38 PM

                                                                    Pre-operation checks

                            Securely install the stern drain plugs by tight-  EJU40553
                                                                  Cooling water pilot outlet check
                            ening them until they stop.
                                                                  Make sure that water is discharged from the
                                                                  cooling water pilot outlet while the engine is
                                                                  running. (See page 34 for information on the
                                                                  cooling water pilot outlet.)

                                          1

                              1 Stern drain plug
                            EJU41441
                            Hood check
                            Push down on the rear of the hood and make
                            sure that it is securely closed.      EJU45260
                                                                  Multifunction information center check
                                                                  Make sure that the multifunction information
                                                                  center operates properly. (See page 45 for in-
                                                                  formation on proper operation of the multi-
                                                                  function information center.)
                                                                  EJU43392
                                                                  Shift system check
                                                                  Operate the throttle lever and RiDE lever, and
                                                                  check that the watercraft moves or does not
                                                                  move according to the displayed shift indica-
                                                                  tor. (See page 35 for shift system operation
                            EJU40146                              procedures.)  WARNING! To avoid colli-
                            Post-launch checks                    sions, operate at safe speeds and keep a
                            Perform the post-launch checks in the pre-
                            operation checklist while the watercraft is in
                            the water and the engine is running.
                            To perform the post-launch checks:
                            (1) Launch the watercraft. (See page 80 for
                                information on launching the watercraft.)
                            (2) Perform the checks and make sure that
                                there are no malfunctioning items or oth-
                                er problems.

                                                                                                   77

| 78 79 80 81 82 83 84 85 86 87 88 |