Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-12-86
P. 67

    UF3V12E0.book  Page 61  Wednesday, June 3, 2020  2:38 PM

                                                                     Equipment operation

                                hood is securely closed before using the
                                watercraft.

                            EJU45291
                            Optional part mounting bracket
                            A mounting  bracket  for installing optional
                            parts is located near the port (left) side of the
                            multifunction information center.

                                     1

                              1 Optional part mounting bracket
                              Load limit:
                                1.0 kg (2.2 lb)

                                                                                                   61

| 62 63 64 65 66 67 68 69 70 71 72 |