Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 102 - LIT-18626-12-86
P. 102

    UF3V12E0.book  Page 96  Wednesday, June 3, 2020  2:38 PM

                            Maintenance

                            EJU33758                              nance not covered by this owner’s/operator’s
                                       Maintenance
                                                                  manual.
                            Periodic  checks and  lubrication will keep  EJU42023
                            your watercraft in the safest and most effi-  Removing and installing the engine
                            cient condition  possible. Therefore, make  cover
                            sure to carry out the periodic maintenance.  The engine cover is removable.
                            Safety is an obligation of the watercraft own-  To remove the engine cover:
                            er. Proper maintenance must be carried out  (1) Remove the seats. (See page 54 for seat
                            to keep the exhaust emission and sound lev-  removal and installation procedures.)
                            els within the regulated limits. The most im-  (2) Remove the engine cover screws.
                            portant points of watercraft inspection  and
                            lubrication are explained on the following pa-
                            ges.
                            See a Yamaha dealer for genuine Yamaha re-
                            placement parts and  optional accessories
                            designed for your watercraft.
                            Remember, failures that are the result of the
                            installation of parts or accessories which are
                                                                                                  1
                            not qualitatively equivalent  to genuine
                            Yamaha parts are not covered by the limited
                                                                   1 Engine cover screw
                            warranty.
                            Maintenance, replacement, or repair of  (3) Lift up the engine cover to remove it.
                            the emission control devices and system
                            may be performed by any marine SI engine
                            repair  establishment or individual.  War-
                            ranty repair, however, must be performed
                            at an authorized Yamaha  marine dealer-
                            ship.
                            EWJ00312

                            Be sure to turn off the engine when you                             1
                            perform maintenance  unless otherwise
                            specified. If you are not familiar with ma-  1 Engine cover
                            chine servicing, this work should be done
                            by a Yamaha dealer or other qualified me-
                            chanic.

                            A service  manual is  available for  purchase
                            through a  Yamaha dealer  for owners  who
                            have the mechanical skills, tools, and other
                            equipment necessary to perform  mainte-

                            96

| 97 98 99 100 101 102 103 104 105 106 107 |