Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 81 - LIT-18626-12-86
P. 81

    UF3V12E0.book  Page 75  Wednesday, June 3, 2020  2:38 PM

                                                                    Pre-operation checks

                            than 15 seconds without supplying water,  and down properly and that the trim setting
                            otherwise the engine could overheat.  indicator and displayed setting level change
                                                                  according to the operation of the switches.
                            Check the start switch, the engine stop
                                                                  (See page 45 for information on turning on
                            switch, and  the engine shut-off  switch for
                                                                  the multifunction information center without
                            proper operation. (See pages 31 to 31 for in-
                                                                  starting the engine and page 37 for informa-
                            formation on operating each switch.)
                                                                  tion on the electric trim system.)
                                               1  2   3

                                                                    0
                                           4
                                                    5
                              1 Clip
                                                                  EJU40102
                              2 Engine shut-off switch
                                                                  Storage compartment checks
                              3 Start switch
                                                                  Make sure  that the storage  compartments
                              4 Engine stop switch
                                                                  are not damaged and that water has not col-
                              5 Engine shut-off cord (lanyard)
                                                                  lected in the compartments. (See page 57 for
                            To check the operation of the switches:  information on the storage compartments.)
                            (1) If the lock mode is selected for  the  EJU41082
                                Yamaha Security System setting, select  Fire extinguisher holder, cover, and band
                                the unlock mode. (See  page  30  for  checks
                                                                  Make sure that the fire extinguisher holder,
                                Yamaha Security System setting proce-
                                                                  cover, and band are not damaged and that
                                dures.)
                                                                  the cover is securely held in place using the
                            (2) Push the start switch to make sure that
                                                                  band. (See page 60 for information on the fire
                                the engine starts.
                                                                  extinguisher holder, cover, and band.)
                            (3) As soon as the  engine  starts  running,
                                push the  engine stop  switch to make
                                sure that the engine stops immediately.
                            (4) Restart the engine, and then pull the en-
                                gine shut-off cord (lanyard) to  remove
                                the clip from the engine shut-off switch
                                to make sure that the engine stops im-
                                mediately.
                            EJU45370
                            Electric trim system check
                            Turn on the multifunction information center,
                            and then operate the “TRIM/T.D.E.” switch-
                            es. Check that the jet thrust nozzle moves up

                                                                                                   75

| 76 77 78 79 80 81 82 83 84 85 86 |