Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 93 - LIT-18626-12-87
P. 93

    UF3Y14E0.book  Page 87  Friday, June 12, 2020  10:50 AM

                                                                                 Maintenance

                            EJU43101
                            Periodic maintenance chart
                            The periodic maintenance chart gives general guidelines for periodic maintenance. Have a
                            Yamaha dealer perform the checks in the following chart. However, maintenance may need
                            to be performed more frequently depending on your operating conditions. If you have any
                            questions, consult a Yamaha dealer.
                            This “√” mark indicates items to be checked and serviced by a Yamaha dealer.
                                                                   Initial    Thereafter every
                                                                                   100    200
                                                                         50 hours
                                   Item             Operation              or 12   hours or  hours or   Page
                                                                  10 hours         12      24
                                                                          months   months  months
                                                                            *1
                                                                                   *1      *1
                                              Check fuel hoses and
                             Fuel line                                              √            —
                                              clamps
                             Fuel filler cap/Wa-  Check O-rings for cracks          √
                             ter separator    and deformation                                    —
                                              Check installation and
                             Fuel tank                                              √            —
                                              straps
                                              Check for clogs and dam-
                             Water inlet strainer                                   √            —
                                              age
                                              Check for damage and
                             Cooling water hos-  leakage, and check                 √            —
                             es
                                              clamps
                             Engine oil       Replace                √              √            89
                             Oil filter       Replace                               √            89
                             Spark plugs      Check                  √              √            —
                                              Check state of charge,
                             Battery                                                √            —
                                              terminals and bands
                             Battery leads    Check terminals                       √            —
                                              Check operation and for
                             Steering master                         √              √            —
                                              looseness
                                              Check exterior and con-
                             Steering cable                                         √            —
                                              nections, and lubricate
                             Shift lever (EX   Check exterior and con-              √
                             SPORT)           nections, and lubricate                            —
                             Shift cable and re-
                             verse gate (EX   Check exterior and con-               √            —
                             SPORT)           nections, and lubricate
                             Shift rod and reverse
                             gate (EX DELUXE /   Check exterior and con-            √            —
                             EX LIMITED)      nections, and lubricate
                                              Check for damage and
                             Air filter element                                     √            —
                                              dirt
                                              Check for damage, and
                             Air intake hoses                                       √            —
                                              check clamps

                                                                                                   87

| 88 89 90 91 92 93 94 95 96 97 98 |