Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-12-87
P. 42

    UF3Y14E0.book  Page 36  Friday, June 12, 2020  10:50 AM

                            Watercraft operation

                            EJU43154                                 reverse, and the “R” (reverse) shift indi-
                            Shift system (EX DELUXE / EX
                                                                     cator will be displayed.
                            LIMITED)
                            EWJ01773
                                                                                      1
                             Make sure that there are no obstacles or
                              people behind you before  shifting  into
                              reverse.
                             Do not touch the reverse gate while the
                              RiDE lever is being operated, otherwise
                              you could be pinched.
                             If the RiDE  lever and throttle lever are
                              being operated at the same time, do not
                                                                   1 RiDE lever
                              release only the RiDE lever. Otherwise,
                              the watercraft  could accelerate more
                              quickly than expected, which may lead                      1
                              to an accident.

                            The RiDE lever and throttle lever can be oper-
                            ated to change the forward or rearward
                            movement of the watercraft only when the
                            engine is running.  When the  RiDE  lever is
                            squeezed, the reverse gate lowers and de-                           2
                            flects the water jet being discharged from the
                            jet thrust nozzle so that the watercraft moves  1 Reverse gate
                            in reverse or is in neutral. When the throttle le-  2 Reverse position
                            ver is squeezed, the reverse gate rises and        1
                            the watercraft moves forward.
                            TIP:
                             This  model is equipped with a function
                              which limits the engine speed in reverse.
                             When the  engine is started,  the reverse
                              gate automatically moves to the neutral po-
                              sition.
                            To shift into reverse:
                            (1) Release the throttle lever.
                                                                   1 “R” (Reverse position)
                            (2) Squeeze the  RiDE lever. The reverse
                                                                  To shift into neutral from reverse:
                                gate will lower, the engine speed will in-
                                                                  Release the RiDE lever. The reverse gate will
                                crease, the watercraft will start moving in
                                                                  automatically return to the  neutral position

                            36

| 37 38 39 40 41 42 43 44 45 46 47 |