Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 90 - LIT-18626-12-87
P. 90

    UF3Y14E0.book  Page 84  Friday, June 12, 2020  10:50 AM

                            Care and storage

                             Steering cable (jet thrust nozzle end)   EX DELUXE / EX LIMITED: Shift rod (re-
                                                                   verse gate end) and ball joint

                             EX SPORT: Shift cable (reverse gate end)
                              and ball joint

                                                                  TIP:
                                                                  Disconnect the shift rod from the ball joint be-
                                                                  fore lubricating.
                                                                  EJU44781
                                                                  Rustproofing
                                                                  Rustproofing the hull, deck, and engine
                                                                  Spray metallic parts of the hull, deck, and en-
                                                                  gine with a rust inhibitor such as Yamalube
                                                                  Silicone Protectant & Lubricant.
                                                                  Rustproofing the internal engine compo-
                                                                  nents
                                                                  Rustproof the  internal engine components
                            TIP:                                  with a rust inhibitor such as Yamalube Stor-
                            Disconnect the shift cable from the ball joint  Rite Engine Fogging Oil.
                            before lubricating.                   To rustproof the internal engine components:
                                                                  (1) Remove the seat  and fire  extinguisher
                                                                     holder. (See page 44 for seat  removal
                                                                     and installation procedures and page 49
                                                                     for information on  the fire extinguisher
                                                                     holder.)
                                                                  (2) Remove the plastic tie that is fastening
                                                                     the fuel hose to the holder on the star-
                                                                     board side of the air filter case.

                            84

| 85 86 87 88 89 90 91 92 93 94 95 |