Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 38 - LIT-18626-12-87
P. 38

    UF3Y14E0.book  Page 32  Friday, June 12, 2020  10:50 AM

                            Control function operation

                            will not start. Also, the starter motor could  EJU43342
                                                                  RiDE lever (EX DELUXE / EX LIMITED)
                            be damaged. [ECJ01041]
                                                                  When the RiDE lever is squeezed, the reverse
                                                                  gate lowers and the watercraft starts moving
                                                     1
                                                                  in reverse. If the watercraft is moving forward,
                                                                  the watercraft gradually slows down until it
                                                                  stops, and then the watercraft starts moving
                                                                  in reverse.

                                                                                      1

                              1 Start switch
                            The engine will not start under any of the fol-
                            lowing conditions:
                             Clip is removed  from  the engine  shut-off
                              switch.
                             Throttle lever is squeezed.          1 RiDE lever
                             Throttle lever is malfunctioning.
                                                                  When the RiDE lever is released, it automati-
                             EX DELUXE / EX LIMITED: RiDE lever is
                                                                  cally returns to its fully closed (idle) position
                              squeezed.
                                                                  and the reverse gate moves to the neutral po-
                             EX DELUXE / EX LIMITED: RiDE lever is
                                                                  sition.
                              malfunctioning.
                                                                  EJU31262
                            EJU31212                              Steering system
                            Throttle lever                        By turning the handlebars in the direction you
                            The throttle lever increases the engine speed
                                                                  wish to travel, the angle of the jet thrust noz-
                            when the lever is squeezed.
                                     1

                              1 Throttle lever
                            The throttle lever returns automatically to its
                            fully closed (idle) position when released.

                            32

| 33 34 35 36 37 38 39 40 41 42 43 |