Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-12-87
P. 67

    UF3Y14E0.book  Page 61  Friday, June 12, 2020  10:50 AM

                                                                    Pre-operation checks

                            the watercraft if the battery does not have  right and left fully turned positions of the jet
                            sufficient power to start the engine or if it  thrust nozzle.
                            shows any other signs of decreased pow-
                            er. Loss of battery power may leave you
                            stranded. [EWJ01241]

                                            2

                              1
                              1 Negative (–) battery terminal: Black lead
                              2 Positive (+) battery terminal: Red lead
                            Make sure that the battery is securely held in
                            place.
                            EJU32614
                            Steering system checks
                            Turn the handlebars to the right and left sev-
                            eral times  to make sure that  operation is
                            smooth and  unrestricted throughout  the
                            whole range, and that the free play is not ex-
                            cessive.

                                                                    Difference between fully turned posi-
                                                                    tions of jet thrust nozzle (distances A
                                                                    and B):
                                                                      Maximum 5 mm (0.20 in)
                                                                  EJU32636
                                                                  Reverse system checks (EX SPORT)
                            Turn the handlebars as far as possible to the  EWJ00032
                            right and left to make sure that the jet thrust
                            nozzle moves as the handlebars are turned,  Do not touch  the  reverse  gate while the
                            and that there is no difference between the  shift lever is being operated, otherwise
                                                                  you could be pinched.

                                                                                                   61

| 62 63 64 65 66 67 68 69 70 71 72 |