Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 68 - LIT-18626-12-87
P. 68

    UF3Y14E0.book  Page 62  Friday, June 12, 2020  10:50 AM

                            Pre-operation checks

                            Operate the shift lever several times to make  EJU43213
                                                                  RiDE lever checks (EX DELUXE / EX
                            sure that operation is smooth throughout the
                                                                  LIMITED)
                            whole range. Also, make sure that the reverse
                                                                  Operate the RiDE lever several times to make
                            gate moves up and down according to the
                                                                  sure that operation is smooth throughout the
                            operation of the shift lever and that the gate
                                                                  whole range. Also, make sure that the RiDE
                            makes contact with the stoppers. (See page
                                                                  lever returns automatically to its fully closed
                            35 for reverse system operation.)
                                                                  position when released.

                                                                  EJU42181
                                                                  Throttle lever checks
                                                                  Operate the throttle lever several times to
                                                                  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the
                                                                  throttle lever returns automatically to its fully
                                                                  closed (idle) position when released.

                                                                  EJU32664
                                                     1            Engine shut-off cord (lanyard) check
                                                                  Make sure that the engine shut-off cord (lan-
                              1 Stopper                           yard) is not damaged. If the cord is damaged,
                                                                  replace it.  WARNING! Never try to repair
                                                                  the engine shut-off cord (lanyard) or tie it
                                                                  together. The  engine  shut-off cord (lan-
                                                                  yard) may not pull free when the operator

                            62

| 63 64 65 66 67 68 69 70 71 72 73 |