Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 79 - LIT-18626-12-87
P. 79

    UF3Y14E0.book  Page 73  Friday, June 12, 2020  10:50 AM

                                                                                      Operation

                            Make sure that there are no obstacles or peo-  be displayed and the watercraft will stop in its
                            ple behind you before shifting into reverse.  current location. (See page 36 for shift sys-
                            TIP:                                  tem operation procedures.)
                            This model is  not equipped with  a  neutral       1
                            function.
                            Operating in reverse (EX DELUXE / EX
                            LIMITED)
                            When the RiDE lever is squeezed, the “R” (re-
                            verse) shift indicator will be displayed and the
                            watercraft will move in reverse. (See page 36
                            for shift system operation procedures.)

                                         1
                                                                   1 “N” (Neutral position)

                              1 “R” (Reverse position)

                                                                  EJU36087
                                                                  Boarding the watercraft
                                                                  EWJ01112

                                                                  Be sure the operator and any passengers
                                                                  have practiced boarding from the water
                                                                  while still close to shore before riding. A
                                                                  person who has made many unsuccessful
                                                                  attempts to get back on the watercraft
                            Make sure that there are no obstacles or peo-
                                                                  may become fatigued and suffer from ex-
                            ple behind you before shifting into reverse.
                                                                  posure, increasing the  risk of injury and
                            TIP:                                  drowning.
                            This model is equipped with a function which
                                                                  Board the watercraft in water free from
                            limits the engine speed in reverse.
                                                                  weeds and debris and at least 60 cm (2 ft)
                            Operating in neutral (EX DELUXE / EX
                            LIMITED)                              deep  from the bottom of  the watercraft.
                            When the RiDE lever is squeezed lightly and  NOTICE: Never run the engine in water
                            released, the “N” (neutral) shift indicator will  that is less than 60 cm (2 ft) deep from the

                                                                                                   73

| 74 75 76 77 78 79 80 81 82 83 84 |