Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-12-87
P. 49

    UF3Y14E0.book  Page 43  Friday, June 12, 2020  10:50 AM

                                                                     Instrument operation

                            higher speeds could result in severe en-  the hour meter and error code alternately at
                            gine damage. [ECJ00042]               3-second intervals.
                                                                                         1

                                                                   1 Error code
                            EJU44690
                            Check engine warning                  If the check engine warning is activated, im-
                            If a sensor malfunction or a short circuit is de-
                                                                  mediately reduce the engine speed, return to
                            tected, the check engine  warning  indicator
                                                                  shore, and have a Yamaha dealer check the
                            and the “WARNING” indicator light blink, and
                                                                  engine.
                            the buzzer sounds intermittently for 30 sec-
                            onds.

                            If the engine is stopped after the check en-
                            gine warning is activated,  the tachometer
                            portion of the information display will show

                                                                                                   43

| 44 45 46 47 48 49 50 51 52 53 54 |