Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 96 - LIT-18626-12-87
P. 96

    UF3Y14E0.book  Page 90  Friday, June 12, 2020  10:50 AM

                            Specifications

                            EJU45432                                Ignition system:
                                      Specifications                  T.C.I.
                            Watercraft capacity:                    Spark plug (NGK):
                              Maximum people on board:                CR9EB
                                3 person                            Spark plug gap:
                              Maximum load capacity:                  0.7–0.8 mm (0.028–0.031 in)
                                225 kg (496 lb)                     Battery capacity:
                            Dimensions and weight:                    12 V, 18 Ah
                              Length:                               Battery type:
                                3.13 m (123.2 in) (EX)                YTX20L-BS
                                3.14 m (123.6 in) (EX SPORT / EX DELUXE/   Charging system:
                                EX LIMITED)                           Flywheel magneto
                              Width:                              Drive unit:
                                1.13 m (44.5 in)                    Propulsion system:
                              Height:                                 Jet pump
                                1.15 m (45.3 in)                    Jet pump type:
                              Dry weight:                             Axial flow, single stage
                                262 kg (578 lb) (EX)                Impeller rotation:
                                265 kg (584 lb) (EX SPORT)            Counterclockwise
                                272 kg (600 lb) (EX DELUXE)         Jet thrust nozzle angle:
                                273 kg (602 lb) (EX LIMITED)          24+24 °
                            Performance:                          Fuel and oil:
                              Maximum fuel consumption:             Recommended fuel:
                                29.2 L/h (7.7 US gal/h, 6.4 Imp.gal/h)  Regular unleaded gasoline
                              Cruising range at full throttle:      Minimum octane rating (PON):
                                1.71 hour                             86
                              Trolling speed:                       Minimum octane rating (RON):
                                1500 ±100 r/min                       90
                            Engine:                                 Recommended engine oil:
                              Engine type:                            YAMALUBE 4W or 4-stroke motor oil
                                Liquid cooled 4-stroke, DOHC
                              Number of cylinders:
                                3
                              Engine displacement:
                                1049 cm³                            Recommended engine oil type SAE:
                              Bore × stroke:                          SAE 10W-30, 10W-40, 20W-40, 20W-50
                                82.0 × 66.2 mm (3.23 × 2.61 in)     Recommended engine oil grade API:
                              Compression ratio:                      API SG, SH, SJ, SL
                                11.0 : 1                            Fuel tank total capacity:
                              Valve clearance-intake (cold):          50 L (13.2 US gal, 11.0 Imp.gal)
                                0.15–0.22 mm (0.0059–0.0087 in)     Engine oil quantity with oil filter replacement:
                              Valve clearance-exhaust (cold):         3.4 L (3.59 US qt, 2.99 Imp.qt)
                                0.26–0.32 mm (0.0102–0.0126 in)     Engine oil quantity without oil filter replacement:
                              Lubrication system:                     3.2 L (3.38 US qt, 2.82 Imp.qt)
                                Dry sump                            Engine oil total quantity:
                              Cooling system:                         3.7 L (3.91 US qt, 3.26 Imp.qt)
                                Water
                              Starting system:
                                Electric

                            90

| 91 92 93 94 95 96 97 98 99 100 101 |