Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 40 - LIT-18626-12-87
P. 40

    UF3Y14E0.book  Page 34  Friday, June 12, 2020  10:50 AM

                            Control function operation

                            If water has collected in the water separator,
                            drain it by loosening the drain screw.

                                       1

                                       2

                              1 Water separator
                              2 Drain screw
                            To drain water from the water separator:
                            (1) Place a drain pan or dry cloth under the
                                water separator.
                            (2) Gradually loosen the drain screw to drain
                                the water. Catch the draining water in the
                                drain pan or soak it up with the dry cloth
                                so that it does not spill into the engine
                                compartment. If any water spills into the
                                watercraft, be sure to wipe it up with a
                                dry cloth.
                            (3) Securely tighten the drain screw until it
                                stops.

                            34

| 35 36 37 38 39 40 41 42 43 44 45 |