Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 71 - LIT-18626-12-87
P. 71

    UF3Y14E0.book  Page 65  Friday, June 12, 2020  10:50 AM

                                                                    Pre-operation checks

                            EJU40146                              EJU43392
                            Post-launch checks                    Shift system check (EX DELUXE / EX
                            Perform the post-launch checks in the pre-  LIMITED)
                            operation checklist while the watercraft is in  Operate the throttle lever and RiDE lever, and
                            the water and the engine is running.  check that the watercraft moves or does not
                            To perform the post-launch checks:    move according to the displayed shift indica-
                            (1) Launch the watercraft. (See page 67 for  tor. (See page 36 for shift system operation
                                information on launching the watercraft.)  procedures.)  WARNING! To avoid colli-
                            (2) Perform the checks and make sure that  sions, operate at safe speeds and keep a
                                there are no malfunctioning items or oth-  safe distance away from people, objects,
                                er problems.                      and other watercraft. [EWJ01860]
                            EJU40553
                            Cooling water pilot outlet check                   1                  2
                            Make sure that water is discharged from the
                            cooling water pilot outlet while the engine is
                                                                                                  3
                            running. (See page 33 for information on the
                            cooling water pilot outlet.)                                          4

                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                                                                  EJU40172
                                                                  Engine idling speed check
                                                                  Start the engine and warm it up. Use the ta-
                            EJU32715
                            Multifunction information center check  chometer in the multifunction  information
                            Make sure that the multifunction information  center to make sure  that the engine  idling
                            center operates properly. (See page 39 for in-  speed is not significantly above or below the
                            formation on proper operation of the multi-  specified range.
                            function information center.)
                                                                    Engine idling speed:
                                                                      1500 ±100 r/min

                                                                                                   65

| 66 67 68 69 70 71 72 73 74 75 76 |