Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 91 - LIT-18626-12-87
P. 91

    UF3Y14E0.book  Page 85  Friday, June 12, 2020  10:50 AM

                                                                           Care and storage

                            (3) Release the hooks on the port side of the  engine is hot. The sprayed substance
                                air filter case, and  remove the air filter  or propellants could catch fire. [EWJ00262]
                                case cover.

                                         2
                                                             3
                              1
                                                             4
                                                             5               1

                                                                   1 Intake opening
                                                                  (5) Place the air filter case cover in its origi-
                                                                     nal position, and then fit the hooks onto
                                                                     the cover.
                                                                  TIP:
                                                                  Make sure that the air filter case cover is se-
                                                                  curely installed.
                                                                  (6) Fasten the fuel hose to the holder using
                                                                     the plastic tie.
                                                                  (7) Make sure that the area around the wa-
                              1 Hook                                 tercraft is clear, and then start the engine
                              2 Air filter case cover                in a well-ventilated area and let it run at
                              3 Fuel hose                            idle for 15 seconds. (See page 31 for in-
                              4 Holder
                                                                     formation on starting the engine.)
                              5 Plastic tie
                                                                  (8) Stop the engine.
                            (4) Spray a rust inhibitor such as Yamalube  (9) Securely install the fire extinguisher hold-
                                Stor-Rite Engine Fogging Oil into the in-  er and seat in their original positions.
                                take opening for 3 seconds. WARNING!
                                Do not spray flammable rust inhibitor
                                products on engine surfaces while the

                                                                                                   85

| 86 87 88 89 90 91 92 93 94 95 96 |