Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-88
P. 69

    UF4L12E0.book  Page 63  Thursday, June 4, 2020  2:02 PM

                                                                    Pre-operation checks

                            EJU43392
                            Shift system check
                            Operate the throttle lever and RiDE lever, and
                            check that the watercraft moves or does not
                            move according to the displayed shift indica-
                            tor. (See page 34 for shift system operation
                            procedures.)  WARNING! To avoid colli-
                            sions, operate at safe speeds and keep a
                            safe distance away from people, objects,
                            and other watercraft. [EWJ01860]
                                         1
                                                             2

                                                             3

                                                             4

                              1 Shift indicator
                              2 “F” (Forward position)
                              3 “N” (Neutral position)
                              4 “R” (Reverse position)
                            EJU40172
                            Engine idling speed check
                            Start the engine and warm it up. Use the ta-
                            chometer in the multifunction  information
                            center to make  sure  that the engine  idling
                            speed is not significantly above or below the
                            specified range.

                              Engine idling speed:
                                1500 ±100 r/min

                                                                                                   63

| 64 65 66 67 68 69 70 71 72 73 74 |