Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-12-88
P. 64

    UF4L12E0.book  Page 58  Thursday, June 4, 2020  2:02 PM

                            Pre-operation checks

                            EJU32424                              EJU41561
                            Water separator check                 Engine oil level check
                            Make sure that no water has collected in the  Make sure that the engine oil level is between
                            water separator. If water has collected in the  the minimum and maximum level marks on
                            water separator, drain it. (See page 32 for in-  the dipstick attached to the oil tank filler cap.
                            formation on draining the water separator.)  (See page 50 for information on checking the
                                                                  engine oil level.)

                                       1
                                                                                                 1

                              1 Water separator
                            EJU40182                               1 Oil tank filler cap/Dipstick
                            Engine unit check
                            Check the exterior of the engine unit for dam-
                            age or other problem.

                                                                          1    2      3

                                                                   1 Dipstick
                                                                   2 Maximum level mark
                                                                   3 Minimum level mark
                                                                  EJU32456
                                                                  Bilge water check
                                                                  Make sure that no bilge water has collected in
                                                                  the engine compartment. If bilge water has
                                                                  collected in the engine compartment, drain it.
                                                                  (See page 52 for information on draining the
                                                                  bilge water.)
                                                                  EJU32486
                                                                  Battery checks
                                                                  Make sure that the battery terminals are not
                                                                  damaged and that the battery leads are con-
                                                                  nected properly. WARNING! Never operate

                            58

| 59 60 61 62 63 64 65 66 67 68 69 |