Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 92 - LIT-18626-12-88
P. 92

    UF4L12E0.book  Page 86  Thursday, June 4, 2020  2:02 PM

                            Specifications

                            EJU45432                                Spark plug gap:
                                      Specifications                  0.7–0.8 mm (0.028–0.031 in)
                            Watercraft capacity:                    Battery capacity:
                              Maximum people on board:                12 V, 18 Ah
                                3 person                            Battery type:
                              Maximum load capacity:                  YTX20L-BS
                                225 kg (496 lb)                     Charging system:
                            Dimensions and weight:                    Flywheel magneto
                              Length:                             Drive unit:
                                3.14 m (123.6 in)                   Propulsion system:
                              Width:                                  Jet pump
                                1.13 m (44.5 in)                    Jet pump type:
                              Height:                                 Axial flow, single stage
                                1.15 m (45.3 in)                    Impeller rotation:
                              Dry weight:                             Counterclockwise
                                245 kg (540 lb)                     Jet thrust nozzle angle:
                            Performance:                              24+24 °
                              Maximum fuel consumption:           Fuel and oil:
                                33.1 L/h (8.7 US gal/h, 7.3 Imp.gal/h)  Recommended fuel:
                              Cruising range at full throttle:        Regular unleaded gasoline
                                1.51 hour                           Minimum octane rating (PON):
                              Trolling speed:                         86
                                1500 ±100 r/min                     Minimum octane rating (RON):
                            Engine:                                   90
                              Engine type:                          Recommended engine oil:
                                Liquid cooled 4-stroke, DOHC          YAMALUBE 4W or 4-stroke motor oil
                              Number of cylinders:
                                3
                              Engine displacement:
                                1049 cm³
                              Bore × stroke:                        Recommended engine oil type SAE:
                                82.0 × 66.2 mm (3.23 × 2.61 in)       SAE 10W-30, 10W-40, 20W-40, 20W-50
                              Compression ratio:                    Recommended engine oil grade API:
                                11.0 : 1                              API SG, SH, SJ, SL
                              Valve clearance-intake (cold):        Fuel tank total capacity:
                                0.15–0.22 mm (0.0059–0.0087 in)       50 L (13.2 US gal, 11.0 Imp.gal)
                              Valve clearance-exhaust (cold):       Engine oil quantity with oil filter replacement:
                                0.26–0.32 mm (0.0102–0.0126 in)       3.4 L (3.59 US qt, 2.99 Imp.qt)
                              Lubrication system:                   Engine oil quantity without oil filter replacement:
                                Dry sump                              3.2 L (3.38 US qt, 2.82 Imp.qt)
                              Cooling system:                       Engine oil total quantity:
                                Water                                 3.7 L (3.91 US qt, 3.26 Imp.qt)
                              Starting system:
                                Electric
                              Ignition system:
                                T.C.I.
                              Spark plug (NGK):
                                CR9EB

                            86

| 87 88 89 90 91 92 93 94 95 96 97 |