Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-12-88
P. 67

    UF4L12E0.book  Page 61  Thursday, June 4, 2020  2:02 PM

                                                                    Pre-operation checks

                            (2) As soon as the  engine  starts  running,  er dealer to obtain one meeting the proper
                                push the  engine stop  switch to make  specifications.
                                sure that the engine stops immediately.
                                                                    Fire extinguisher:
                            (3) Restart the engine, and then pull the en-
                                                                      Classification:
                                gine shut-off cord (lanyard) to  remove  5-B (B-1)
                                the clip from the engine shut-off switch  Capacity:
                                to make sure that the engine stops im-  2 lb or more
                                mediately.
                                                                  EJU40122
                            EJU40102
                            Storage compartment checks            Safety equipment check
                            Make  sure that  the storage compartments  Check that safety equipment meeting the ap-
                            are not damaged and that water has not col-  plicable regulations is on board.
                                                                  EJU32353
                            lected in the compartments. (See page 44 for  Hull and deck check
                            information on the storage compartments.)  Check the hull and deck for damage or other
                            EJU44670                              problem.
                            Fire extinguisher holder checks
                                                                  EJU32657
                            Make sure that the fire extinguisher holder is  Jet intake checks
                            installed  in the  correct direction and  is not  Make sure that the jet intake is not damaged
                            damaged. (See page  47  for information  on  or clogged with weeds or debris. If the jet in-
                            the fire extinguisher holder.)        take is clogged, clean it. (See page 90 for in-
                            EJU44621                              formation on the jet intake.)
                            Fire extinguisher check
                                                                  EJU43221
                            Check that there is a full fire extinguisher on  Jet thrust nozzle and reverse gate check
                            board.                                Check the jet thrust nozzle and reverse gate
                                                                  for damage or other problem.
                                                                  EJU44250
                                                                  Stern drain plug checks
                                                                  Loosen the stern drain plugs and  remove
                                                                  them, and then make sure that the plugs and
                                                                  O-rings on the plugs are not damaged and
                                                                  that there is no foreign material on the
                                                                  threads or O-rings on  the plugs.  NOTICE:
                                                                  Before installing  the stern drain plugs,
                                                                  clean the  drain plug threads and the  O-
                                                                  rings on the plugs to remove any foreign
                            To check  the  fire extinguisher, see the  in-
                                                                  materials, such as dirt or sand. Otherwise,
                            structions supplied  by the fire extinguisher
                                                                  the stern drain plugs could be damaged,
                            manufacturer. Always keep the fire extin-
                                                                  allowing water to enter the engine com-
                            guisher stored in the holder.
                                                                  partment. Check the O-rings on the stern
                            Always carry a fire extinguisher on board. A
                                                                  drain plugs and make sure that the plugs
                            fire extinguisher is not standard  equipment
                                                                  are tightened securely before launching
                            with this watercraft. If you do not have one,
                                                                  the  watercraft. Otherwise, water may
                            contact a Yamaha dealer or a fire extinguish-
                                                                                                   61

| 62 63 64 65 66 67 68 69 70 71 72 |