Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-12-88
P. 42

    UF4L12E0.book  Page 36  Thursday, June 4, 2020  2:02 PM

                            Watercraft operation

                            TIP:
                            If the RiDE lever is squeezed while the throttle
                            lever is squeezed, the  watercraft  will  slow
                            down, and once stopped, move in reverse.
                            To shift into neutral from forward:
                            (1) Release the throttle lever.
                            (2) Lightly squeeze and release the RiDE le-
                                ver. The “N” (neutral) shift indicator will
                                be displayed.

                                         1

                              1 “N” (Neutral position)
                            TIP:
                            If the RiDE lever is squeezed continuously,
                            the reverse gate will move to the reverse po-
                            sition.

                            36

| 37 38 39 40 41 42 43 44 45 46 47 |