Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-12-88
P. 49

    UF4L12E0.book  Page 43  Thursday, June 4, 2020  2:02 PM

                                                                     Equipment operation

                            breaks, the watercraft could fall, which  step breaks, the watercraft  could  fall,
                            could result in severe injury. [EWJ00022]  which could result in severe injury. [EWJ01212]

                                                                                               1
                                                           1

                              1 Handgrip                           1 Reboarding step
                            EJU37382
                            Reboarding grip
                            The reboarding grip is used when boarding
                            the watercraft from the water.

                                                          1

                                                                  ECJ00743

                                                                  Use the reboarding step only to board the
                              1 Reboarding grip                   watercraft in the water. Do not use the re-
                                                                  boarding step for any other purpose. The
                            EJU34865
                            Reboarding step                       watercraft can be damaged.
                            The reboarding step is used to assist in re-
                            boarding the watercraft from the water.
                            When boarding the watercraft, push the re-
                            boarding step down until it stops. The step
                            returns automatically to its original position
                            when released. WARNING! Do not use the
                            reboarding step to lift the watercraft. The
                            reboarding step is not designed to support
                            the watercraft’s weight. If the reboarding

                                                                                                   43

| 44 45 46 47 48 49 50 51 52 53 54 |