Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 65 - LIT-18626-12-88
P. 65

    UF4L12E0.book  Page 59  Thursday, June 4, 2020  2:02 PM

                                                                    Pre-operation checks

                            the watercraft if the battery does not have  right and left fully turned positions of the jet
                            sufficient power to start the engine or if it  thrust nozzle.
                            shows any other signs of decreased pow-
                            er. Loss of battery power may leave you
                            stranded. [EWJ01241]

                                            2

                              1
                              1 Negative (–) battery terminal: Black lead
                              2 Positive (+) battery terminal: Red lead
                            Make sure that the battery is securely held in
                            place.
                            EJU32614
                            Steering system checks
                            Turn the handlebars to the right and left sev-
                            eral times  to make sure that  operation is
                            smooth and  unrestricted throughout  the
                            whole range, and that the free play is not ex-
                            cessive.

                                                                    Difference between fully turned posi-
                                                                    tions of jet thrust nozzle (distances A
                                                                    and B):
                                                                      Maximum 5 mm (0.20 in)
                                                                  EJU43213
                                                                  RiDE lever checks
                            Turn the handlebars as far as possible to the  Operate the RiDE lever several times to make
                            right and left to make sure that the jet thrust  sure that operation is smooth throughout the
                            nozzle moves as the handlebars are turned,  whole range. Also, make sure that the RiDE
                            and that there is no difference between the

                                                                                                   59

| 60 61 62 63 64 65 66 67 68 69 70 |