Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-12-88
P. 66

    UF4L12E0.book  Page 60  Thursday, June 4, 2020  2:02 PM

                            Pre-operation checks

                            lever returns automatically to its fully closed  falls off, allowing the watercraft to conti-
                            position when released.               nue to run and cause an accident. [EWJ01221]

                            EJU42181                              EJU40692
                            Throttle lever checks                 Switch checks
                            Operate the throttle lever  several times  to  ECJ01311
                            make sure that operation is smooth through-
                            out the whole range. Also, make sure that the  Do not run the engine over 4000 r/min on
                            throttle lever returns automatically to its fully  land. Also, do not run the engine for more
                            closed (idle) position when released.  than 15 seconds without supplying water,
                                                                  otherwise the engine could overheat.

                                                                  Check the start switch, the engine stop
                                                                  switch,  and the engine  shut-off switch  for
                                                                  proper operation. (See pages 30 to 30 for in-
                                                                  formation on operating each switch.)
                                                                                    1

                                                                                              3

                            EJU32664
                            Engine shut-off cord (lanyard) check                              4
                            Make sure that the engine shut-off cord (lan-
                            yard) is not damaged. If the cord is damaged,
                            replace it.  WARNING! Never try to repair            2        5
                            the engine shut-off cord (lanyard) or tie it
                            together. The engine  shut-off cord (lan-  1 Start switch
                                                                   2 Engine stop switch
                            yard) may not pull free when the operator
                                                                   3 Engine shut-off switch
                                                                   4 Clip
                                                                   5 Engine shut-off cord (lanyard)
                                                                  To check the operation of the switches:
                                                                  (1) Push the start switch to make sure that
                                                                     the engine starts.

                            60

| 61 62 63 64 65 66 67 68 69 70 71 |