Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 86 - LIT-18626-12-88
P. 86

    UF4L12E0.book  Page 80  Thursday, June 4, 2020  2:02 PM

                            Care and storage

                             Steering cable (jet thrust nozzle end)  To rustproof the internal engine components:
                                                                  (1) Remove the seat  and fire  extinguisher
                                                                     holder. (See page 42 for seat  removal
                                                                     and installation procedures and page 47
                                                                     for information on  the fire extinguisher
                                                                     holder.)
                                                                  (2) Remove the plastic tie that is fastening
                                                                     the fuel hose to the holder on the star-
                                                                     board side of the air filter case.
                                                                  (3) Release the hooks on the port side of the
                                                                     air filter case, and remove the air filter
                             Shift rod (reverse gate end) and ball joint  case cover.
                                                                               2
                                                                                                  3
                                                                   1
                                                                                                  4
                                                                                                  5

                            TIP:
                            Disconnect the shift rod from the ball joint be-
                            fore lubricating.
                            EJU44781
                            Rustproofing
                                                                   1 Hook
                            Rustproofing the hull, deck, and engine
                                                                   2 Air filter case cover
                            Spray metallic parts of the hull, deck, and en-
                                                                   3 Fuel hose
                            gine with a rust inhibitor such as Yamalube
                                                                   4 Holder
                            Silicone Protectant & Lubricant.       5 Plastic tie
                            Rustproofing the internal engine compo-
                                                                  (4) Spray a rust inhibitor such as Yamalube
                            nents
                                                                     Stor-Rite Engine Fogging Oil into the in-
                            Rustproof the internal  engine  components
                                                                     take opening for 3 seconds. WARNING!
                            with a rust inhibitor such as Yamalube Stor-
                                                                     Do not spray flammable rust inhibitor
                            Rite Engine Fogging Oil.
                                                                     products on engine surfaces while the
                            80

| 81 82 83 84 85 86 87 88 89 90 91 |