Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 85 - LIT-18626-12-89
P. 85

    UF4R10E0.book  Page 80  Tuesday, August 4, 2020  1:32 PM

                                                                           Trouble recovery

                            (1) Securely attach the towline to the bow  dealer inspect the watercraft. Other-
                                eye of the watercraft being towed.   wise, serious engine damage could
                                                                     result. [ECJ00792]

                                 1

                              1 Bow eye
                            (2) Ride the watercraft with your body
                                weight supported on the riding tray. Hold
                                on to the handlebars in order to balance
                                the watercraft and keep the bow up out
                                of the water. NOTICE: The bow must be
                                kept up out of the water during tow-
                                ing, otherwise water could flood  the
                                engine compartment or water could
                                flow back into the engine, causing se-
                                vere engine damage. [ECJ01331]
                            Tow the watercraft at 8 km/h (5 mph) or less.
                            NOTICE: Tow the watercraft at 8 km/h (5
                            mph) or less, otherwise water could flood
                            the engine  compartment or water could
                            flow back into the engine, causing severe
                            engine damage. [ECJ01322]
                            EJU34736
                            Submerged watercraft
                            If the watercraft is submerged or flooded with
                            water, drain the bilge water from the engine
                            compartment. Then, have a Yamaha dealer
                            service the watercraft as soon as possible.
                            (1) Remove the watercraft from the water.
                            (2) Drain the bilge water from the engine
                                compartment. (See page 41 for informa-
                                tion on draining the bilge water on land.)
                            (3) Have the watercraft serviced  by a
                                Yamaha  dealer as soon  as possible.
                                NOTICE:  Be  sure to have a  Yamaha

                                                                                                   80

| 80 81 82 83 84 85 86 87 88 89 90 |