Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 55 - LIT-18626-12-89
P. 55

    UF4R10E0.book  Page 50  Tuesday, August 4, 2020  1:32 PM

                                                                    Pre-operation checks

                            Make sure that there is the proper amount of  EJU45610
                                                                  Switch checks
                            throttle lever free play when the throttle lever  ECJ01361
                            is in the fully closed (idle) position.
                                                                  Do not run  the engine for  more than 15
                                            1
                                                                  seconds on land without supplying water,
                                                                  otherwise the engine could overheat.

                                                                  Check the start switch, the engine stop/“L-
                                                                  MODE” switch, and the  engine shut-off
                                                                  switch for proper operation. (See pages 27 to
                                                                  27 for information on operating each switch.)

                                                                                             3
                                                                            2
                              1 Throttle lever free play
                                                                       1
                              Throttle lever free play:
                                3.0–6.0 mm (0.12–0.24 in)

                            EJU32664
                            Engine shut-off cord (lanyard) check
                            Make sure that the engine shut-off cord (lan-        5           4
                            yard) is not damaged. If the cord is damaged,
                            replace it.  WARNING! Never try to repair  1 Start switch
                            the engine shut-off cord (lanyard) or tie it  2 Engine shut-off switch
                            together. The engine  shut-off cord (lan-  3 Clip
                            yard) may not pull free when the operator  4 Engine shut-off cord (lanyard)
                            falls off, allowing the watercraft to conti-  5 Engine stop/“L-MODE” switch
                            nue to run and cause an accident. [EWJ01221]  To check the operation of the switches:
                                                                  (1) Push the start switch to make sure that
                                                                     the engine starts.
                                                                  (2) As  soon as the  engine starts running,
                                                                     push the engine stop/“L-MODE” switch
                                                                     to make sure that the engine stops im-
                                                                     mediately.
                                                                  (3) Restart the engine, and then pull the en-
                                                                     gine  shut-off cord (lanyard) to  remove
                                                                     the clip from the engine shut-off switch
                                                                     to make sure that the engine stops im-
                                                                     mediately.
                                                                  EJU41211
                                                                  Storage pouch checks
                                                                  Make sure that the storage pouch is not dam-
                                                                  aged and that water has not collected in the

                                                                                                   50

| 50 51 52 53 54 55 56 57 58 59 60 |