Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-89
P. 69

    UF4R10E0.book  Page 64  Tuesday, August 4, 2020  1:32 PM

                                                                           Care and storage

                                water flows  out continually  from the  water when rinsing the engine or en-
                                cooling water pilot outlet.          gine  compartment as severe engine
                                                                     damage could result. [ECJ00572]
                                                                  (3) Drain  the water  from the engine com-
                                                                     partment. (See page 41 for information
                                                                     on draining the bilge water.)
                                                                  (4) Wipe  the engine  and engine compart-
                                                                     ment with a dry cloth.
                                                                  (5) Wash down the hull, deck, and jet pump
                                                                     with fresh water.
                                                                  (6) Wipe the hull, deck, and jet pump with a
                                                                     dry cloth.
                            (7) Run the engine at idling speed for about  (7) Wipe  all vinyl and rubber components,
                                3 minutes watching the engine condition.  such as the engine compartment seals,
                                If the  engine stops  while flushing,  turn  with  a vinyl  protectant such as Yama-
                                the water supply off immediately  and  clean Vinyl Dressing™.
                                perform the procedure again from step 6.  (8) To minimize corrosion, spray metallic
                                NOTICE: Do not supply water to the   parts of the hull, deck, and engine with a
                                cooling water passages when the en-  rust inhibitor such as Yamalube Silicone
                                gine is not running. The water could  Protectant & Lubricant.
                                flow back through the muffler into the  (9) Allow the engine compartment to air dry
                                engine, causing severe engine  dam-  completely before installing the hood.
                                                                  (10) Securely install the hood in its original
                                age. [ECJ00123]
                            (8) Turn the water supply off.           position.
                            (9) Discharge the remaining water out of the  EJU41634
                                                                  Battery care
                                cooling  water passages by  alternately
                                                                  If the watercraft will not be used for more than
                                squeezing and releasing the throttle lever
                                                                  a month, remove the battery from the water-
                                quickly for 10 to 15 seconds.
                                                                  craft, check it, and then store it in a cool, dry
                            (10) Stop the engine.
                                                                  place.
                            (11) Remove the garden hose adapter, and  EWJ00792
                                then securely install the flushing hose
                                connector cap  by tightening  it until it
                                                                  Battery electrolyte is poisonous and dan-
                                stops.
                                                                  gerous, causing severe burns, etc. Elec-
                            (12) Securely install the  hood in its original
                                                                  trolyte contains sulfuric acid. Avoid
                                position.
                                                                  contact with skin, eyes, or clothing.
                            EJU40737
                            Cleaning the watercraft               Antidotes
                            (1) Remove the hood. (See page 33 for hood  External: Flush with water.
                                removal and installation procedures.)  Internal: Drink large quantities of water or
                            (2) Rinse the engine and engine compart-  milk. Follow with milk of magnesia, beaten
                                ment with a small amount  of  water.  egg, or vegetable oil. Call a physician im-
                                NOTICE: Do not use high-pressure  mediately.
                                                                                                   64

| 64 65 66 67 68 69 70 71 72 73 74 |