Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-12-89
P. 48

    UF4R10E0.book  Page 43  Tuesday, August 4, 2020  1:32 PM

                            Operation and handling requirements

                            EJU45601                              with the steering pole up. Otherwise, the
                                Transporting on a trailer
                                                                  steering pole could be damaged. [ECJ02820]
                            When transporting the watercraft on a trailer,
                            secure the tie downs to the trailer through the
                            bow eye and stern eyes. Use a rubber shock
                            cord to secure the steering pole to the water-
                            craft. NOTICE: Do not attach ropes or tie
                            downs to any part of the watercraft other
                            than the bow eye and stern eyes to secure
                            the watercraft to the trailer. Otherwise, the
                            watercraft may be damaged.  Wrap  the
                            ropes or tie downs with towels  or  rags
                            where they touch the body of the water-
                            craft to avoid scratches or damage.  Do
                            not secure the steering pole with ropes or
                            tie downs and do not secure it to the trail-
                            er. Also, do not  transport the watercraft

                                                                                                 1

                                                                   1 Rubber shock cord

                            43

| 43 44 45 46 47 48 49 50 51 52 53 |