Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 60 - LIT-18626-12-89
P. 60

    UF4R10E0.book  Page 55  Tuesday, August 4, 2020  1:32 PM

                            Operation

                                the jet intake, causing impeller dam-  engine. (See page 27 for information on
                                age and engine overheating. [ECJ00473]  operating the start switch.)

                                           60 cm (2 ft)

                            (2) Attach the engine shut-off cord (lanyard)  EJU45710
                                                                  Stopping the engine
                                to your left wrist, and then attach the clip
                                                                  Release the throttle lever, and then push the
                                to the engine shut-off switch. (See page
                                                                  engine stop/“L-MODE” switch (red button) to
                                27 for information on operating the en-
                                                                  stop the engine.  WARNING! You  need
                                gine shut-off switch.) WARNING! Check
                                                                  throttle to  steer. Shutting the engine off
                                that the engine shut-off cord (lanyard)
                                                                  can cause you to hit an obstacle you are
                                is attached  correctly. If the engine
                                                                  attempting to avoid. A collision could re-
                                shut-off cord (lanyard) is not attached
                                                                  sult in severe injury or death. [EWJ00602]
                                correctly, it may not pull free when the
                                operator falls off, allowing the water-
                                craft to continue to run and cause an
                                accident. [EWJ00582]
                                           1
                                                      2

                                                                  EJU32873
                                                3                 Leaving the watercraft
                                                                  If leaving the watercraft, remove the clip from
                                                                  the  engine shut-off switch  to prevent acci-
                              1 Clip
                              2 Engine shut-off switch
                              3 Engine shut-off cord (lanyard)
                            (3) With the throttle lever released, push the
                                start  switch (green  button) to start  the

                            55

| 55 56 57 58 59 60 61 62 63 64 65 |