Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-12-89
P. 39

    UF4R10E0.book  Page 34  Tuesday, August 4, 2020  1:32 PM

                                                                     Equipment operation

                            To install the hood:                  (2) Push down on the hood latch, and then
                            (1) Position the hood on the deck so that the  turn the knob to the “LOCK” position to
                                two projections at the front of the hood fit  securely lock the hood in place.
                                under the two stays on the deck.
                                                                                                  1

                                                                                                  2

                                                                   1 Hood latch
                                                                   2 Hood latch knob

                                                                  (3) While holding the steering pole, move
                                                                     the lock pin to the stowed position, and
                                                                     then lower the steering pole.

                                                                                                   34

| 34 35 36 37 38 39 40 41 42 43 44 |