Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 33 - LIT-18626-12-89
P. 33

    UF4R10E0.book  Page 28  Tuesday, August 4, 2020  1:32 PM

                                                             Control function operation

                            will not start. Also, the starter motor could  zle is changed, and the direction of the water-
                            be damaged. [ECJ01041]                craft is changed accordingly.

                                                                                           1

                                    1

                              1 Start switch
                            The engine will not start under any of the fol-                       2
                            lowing conditions:
                             Clip is removed  from  the engine  shut-off
                              switch.
                             Throttle lever is squeezed.
                            EJU31212
                            Throttle lever                         1 Handlebar
                            The throttle lever increases the engine speed  2 Jet thrust nozzle
                            when the lever is squeezed.
                                                                  Since the strength of the jet thrust determines
                                                                  the speed and degree of a turn, throttle must
                                                                  always be applied when attempting a turn,
                                                                  except at trolling speed.
                                                        1         The angle of the jet thrust nozzle can be ad-
                                                                  justed to suit operator preference. (See page
                                                                  70 for information on adjusting the jet thrust
                                                                  nozzle angle.)

                              1 Throttle lever
                            The throttle lever returns automatically to its
                            fully closed (idle) position when released.
                            EJU35933
                            Steering system
                            By turning the handlebars in the direction you
                            wish to travel, the angle of the jet thrust noz-

                                                                                                   28

| 28 29 30 31 32 33 34 35 36 37 38 |