Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 36 - LIT-18626-12-89
P. 36

    UF4R10E0.book  Page 31  Tuesday, August 4, 2020  1:32 PM

                            Instrument operation

                            EJU45701                              EJU45631
                                           Meter                  Fuel level warning
                            When the meter is activated, all of the fuel  If the fuel remaining in the fuel tank drops to
                            level meter segments and all indicators come  about 6.0 L (1.59 US gal, 1.32 Imp.gal), the
                            on. After a few seconds, the fuel level meter  lowest fuel level segment blinks.
                            displays the remaining amount of fuel and all
                            indicators go off.

                                  1

                                 2                        3
                                                                  If the fuel level warning is activated, refill the
                                                                  fuel tank as soon as possible. (See page 38
                              1 “WARNING” indicator light         for information on filling the fuel tank.)
                              2 “L-MODE” indicator light          EJU45641
                              3 Fuel level meter                  Indicator lights
                            EJU45620
                            Fuel level meter
                            The fuel level meter shows the amount of fuel  1
                            remaining in the fuel tank. The amount of re-
                            maining fuel is shown using four display seg-
                            ments, which disappear one at a time as the
                            fuel level decreases.
                            TIP:                                      2
                            The accuracy of the fuel level meter varies
                            depending on the operating conditions. Use
                                                                   1 “WARNING” indicator light
                            this function as a reference only.
                                                                   2 “L-MODE” indicator light
                                                                  EJU45650
                                                                  Oil pressure warning
                                                                  If the oil pressure drops significantly,  the
                                                                  “WARNING” indicator light blinks.  At  the
                                                           1

                              1 Fuel level meter

                            31

| 31 32 33 34 35 36 37 38 39 40 41 |