Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 76 - LIT-18626-12-89
P. 76

    UF4R10E0.book  Page 71  Tuesday, August 4, 2020  1:32 PM

                            Maintenance

                                and then tighten the bolt to the specified  EJU45671
                                                                  Adjusting the handlebar position
                                torque.
                                                                  The handlebar can be adjusted to three posi-
                            TIP:                                  tions to  suit the rider’s preference.  Have a
                            The outermost hole in the steering column  Yamaha dealer adjust the position of the han-
                            cannot be used.                       dlebar.

                                  1                     1
                              1 Nozzle angles

                                    1                2

                                    16°

                                                            P1

                                    19°

                                                            P2
                              1 Nozzle angles
                              2 Steering cable pivot bolt positions
                              Standard steering cable pivot bolt posi-
                              tion:
                                P2
                              Tightening torque:
                                Steering cable pivot bolt:
                                  5 N·m (0.5 kgf·m, 3.7 lb·ft)

                            (4) Securely connect the steering cable joint
                                to the steering cable pivot bolt.

                            71

| 71 72 73 74 75 76 77 78 79 80 81 |