Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-12-89
P. 75

    UF4R10E0.book  Page 70  Tuesday, August 4, 2020  1:32 PM

                                                                                 Maintenance

                            (2) Remove the plastic fasteners, and then  (7) Securely install the handlebar cover and
                                remove the handlebar cover.          the plastic fasteners in their original posi-
                                                                     tions.
                                                                  (8) While holding the steering pole, move
                                                                     the lock pin to the stowed position, and
                                                                     then lower the steering pole.
                                                                  EJU3128C
                                                                  Adjusting the jet thrust nozzle angle
                                    1                             The angle of the jet thrust nozzle can be ad-
                                                       2
                                                                  justed to two settings to suit operator prefer-
                                                                  ence.
                                                                  To adjust the jet thrust nozzle angle:
                                                                  (1) Pull back the outer sleeve of the steering
                              1 Plastic fastener
                              2 Handlebar cover                      cable joint, and then disconnect the joint
                                                                     from the steering cable pivot bolt.
                            (3) Turn the handlebars so that the left han-
                                dlebar grip is facing down.
                            (4) Loosen the locknut.
                            (5) Tighten or loosen the adjusting nut until
                                the desired  amount  of friction is  ob-
                                tained.

                                                                                               1

                                                                   1 Steering cable joint
                                                                  (2) Remove the steering cable pivot bolt.
                                                     1

                                        2
                              1 Adjusting nut
                              2 Locknut                                                        2
                            (6) While holding  the adjusting nut with  a
                                wrench, tighten the locknut to the speci-
                                                                          1
                                fied torque.
                              Tightening torque:
                                Locknut:                           1 Steering cable pivot bolt
                                  28 N·m (2.8 kgf·m, 21 lb·ft)     2 Steering column
                                                                  (3) Select the nozzle angle, install the steer-
                                                                     ing cable pivot bolt in the desired posi-
                                                                     tion (P1 or P2) on the steering column,

                                                                                                   70

| 70 71 72 73 74 75 76 77 78 79 80 |