Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 57 - LIT-18626-12-89
P. 57

    UF4R10E0.book  Page 52  Tuesday, August 4, 2020  1:32 PM

                                                                    Pre-operation checks

                            flood the engine compartment and cause  EJU40146
                                                                  Post-launch checks
                            the watercraft to submerge. [ECJ00363]
                                                                  Perform the post-launch checks in the pre-
                                                                  operation checklist while the watercraft is in
                                                                  the water and the engine is running.
                                                                  To perform the post-launch checks:
                                                                  (1) Launch the watercraft. (See page 54 for
                                                                     information on launching the watercraft.)
                                                                  (2) Perform the checks and make sure that
                                                             2       there are no malfunctioning items or oth-
                                                                     er problems.
                                                                  EJU40553
                                                             1    Cooling water pilot outlet check
                              1 Stern drain plug                  Make sure that water is discharged from the
                              2 O-ring
                                                                  cooling water pilot outlet while the engine is
                            Securely install the stern drain plugs by tight-  running. (See page 29 for information on the
                            ening them until they stop.           cooling water pilot outlet.)

                                                            1

                              1 Stern drain plug                  EJU45840
                                                                  Meter check
                            EJU40703
                            Hood check                            Make sure that the meter operates properly.
                            Make sure that the hood is securely closed.  (See page 31 for information on proper oper-
                            (See page 33 for information on the hood.)  ation of the meter.)

                                                                                                   52

| 52 53 54 55 56 57 58 59 60 61 62 |