Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 38 - LIT-18626-12-89
P. 38

    UF4R10E0.book  Page 33  Tuesday, August 4, 2020  1:32 PM

                            Equipment operation

                            EJU40335                              (2) Turn the latch knob to the “OPEN” posi-
                                        Equipment
                                                                     tion, and then pull up on the hood latch
                            EJU3105A
                            Hood                                     to unlatch the hood.
                            The hood is removable.
                            Remove the hood to access the engine com-                             1
                            partment.
                            To remove the hood:                                                   2
                            (1) Lift the steering pole and support it with
                                the lock pin.

                                                                   1 Hood latch
                                                       1           2 Hood latch knob

                              1 Steering pole

                                         1

                                                                  (3) Grasp the hood using the handgrips pro-
                                                                     vided at the front and rear of the hood.
                                                                     Lift the hood up and to the rear to re-
                                                                     move it.
                              1 Lock pin

                                                                                       1

                                                                                                 1

                                                                   1 Handgrip

                            33

| 33 34 35 36 37 38 39 40 41 42 43 |