Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-12-89
P. 42

    UF4R10E0.book  Page 37  Tuesday, August 4, 2020  1:32 PM

                            Equipment operation

                            To close the fire extinguisher holder:
                            (1) Insert the projection into the slot, slide
                                the cover forward, and then secure it
                                with the band.

                                 2
                                                 1

                              1 Projection
                              2 Slot
                            (2) While  holding the  steering pole, move
                                the lock pin to the stowed position, and
                                then lower the steering pole.

                            37

| 37 38 39 40 41 42 43 44 45 46 47 |