Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-12-89
P. 52

    UF4R10E0.book  Page 47  Tuesday, August 4, 2020  1:32 PM

                            Pre-operation checks

                            EJU32282                               If any fuel leakage is found, the fuel sys-
                               Pre-operation check points
                                                                   tem must be repaired by a qualified me-
                            EJU40686
                            Pre-launch checks                      chanic. Improper repairs can make the
                            Perform the pre-launch checks in the pre-op-  watercraft unsafe to operate.
                            eration checklist while the watercraft is  on
                                                                  Make sure that there is no damage, leakage,
                            land.
                                                                  or other problem in the fuel system.
                            To perform the pre-launch checks:
                                                                  Check:
                            (1) Remove the hood. (See page 33 for hood
                                                                   Fuel filler cap and seal for damage
                                removal and installation procedures.)
                                                                   Fuel tank for damage and leakage
                            (2) Perform the checks and make sure that
                                                                   Fuel hoses and joints for damage and leak-
                                there are no malfunctioning items or oth-
                                                                   age
                                er problems.
                                                                   Fuel tank breather hose  for damage and
                            (3) After completing these checks, install the
                                                                   leakage
                                hood in its original position.    EJU36875
                            EJU32334                              Fuel level check
                            Engine compartment check              Check the fuel level in the fuel tank.
                            EWJ00462
                                                                  Add fuel if necessary. (See page 38 for infor-
                                                                  mation on filling the fuel tank.)
                            Failure  to  ventilate the engine compart-
                                                                  EJU32424
                            ment could result in a fire or explosion. Do  Water separator check
                            not start the engine if there is a fuel leak.  Make sure that no water has collected in the
                                                                  water separator. If water has collected in the
                            Ventilate the engine compartment. Leave the
                                                                  water separator, drain it. (See page 29 for in-
                            engine compartment open for a few minutes
                                                                  formation on draining the water separator.)
                            to allow any fuel vapors to escape.
                            Make sure that there is no damage inside the
                            engine compartment.                             1
                                                                            2

                                                                   1 Water separator
                                                                   2 Drain screw
                                                                  EJU40182
                                                                  Engine unit check
                            EJU34215
                            Fuel system checks                    Check the exterior of the engine unit for dam-
                            EWJ00382
                                                                  age or other problem.
                            Leaking fuel can result in fire or explosion.
                             Check for fuel leakage regularly.

                            47

| 47 48 49 50 51 52 53 54 55 56 57 |