Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 74 - LIT-18626-12-89
P. 74

    UF4R10E0.book  Page 69  Tuesday, August 4, 2020  1:32 PM

                            Maintenance

                            EJU33759                              nance not covered by this owner’s/operator’s
                                       Maintenance
                                                                  manual.
                            Periodic  checks and  lubrication will keep  EJU3433A
                            your watercraft in the safest and most effi-  Adjusting the steering friction
                            cient condition  possible. Therefore, make  The amount of friction in the steering can be
                            sure to carry out the periodic maintenance.  adjusted to suit operator preference.
                            Safety is an obligation of the watercraft own-  To adjust the steering friction:
                            er. Proper maintenance must be carried out  (1) Lift the steering pole and support it with
                            to keep the exhaust emission and sound lev-  the lock pin.
                            els within the regulated limits. The most im-
                            portant points of watercraft inspection  and
                            lubrication are explained on the following pa-
                            ges.
                            See a Yamaha dealer for genuine Yamaha re-                      1
                            placement parts and  optional accessories
                            designed for your watercraft.
                            Remember, failures that are the result of the
                            installation of parts or accessories which are
                            not qualitatively equivalent  to genuine
                                                                   1 Steering pole
                            Yamaha parts are not covered by the limited
                            warranty.
                            Maintenance, replacement, or repair of
                            the emission control devices and system            1
                            may be performed by any marine SI engine
                            repair  establishment or individual.  War-
                            ranty repair, however, must be performed
                            at an authorized Yamaha  marine dealer-
                            ship.
                            EWJ00312

                            Be sure to turn off the engine when you  1 Lock pin
                            perform maintenance  unless otherwise
                            specified. If you are not familiar with ma-
                            chine servicing, this work should be done
                            by a Yamaha dealer or other qualified me-
                            chanic.

                            A service  manual is  available for  purchase
                            through a  Yamaha dealer  for owners  who
                            have the mechanical skills, tools, and other
                            equipment necessary to perform  mainte-

                            69

| 69 70 71 72 73 74 75 76 77 78 79 |