Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 59 - LIT-18626-12-89
P. 59

    UF4R10E0.book  Page 54  Tuesday, August 4, 2020  1:32 PM

                                                                                      Operation

                            EJU33172                              will probably need to return to the kneeling
                            Operating positions
                                                                  position to maintain your balance.
                            After you are underway, you may choose to
                            kneel or stand, depending upon watercraft
                            speed, your skill level, and your preference.
                            Here are some guidelines.
                            Kneeling
                            It is easier to maintain your balance when
                            kneeling than when standing. This position is
                            recommended when traveling at sub-planing
                            speeds.  (At  sub-planing speeds, there is a
                            wake, but the watercraft is moving through
                            the water rather than skimming on top of it.)
                                                                  EJU32822
                                                                  Launching the watercraft
                                                                  When launching the watercraft,  make  sure
                                                                  that there are no obstacles around you.
                                                                  If the watercraft is launched from a trailer,
                                                                  someone should make sure that waves do
                                                                  not push the watercraft into the trailer.
                                                                  After the watercraft is in the water,  turn it
                                                                  around so that the bow faces the direction
                                                                  you wish to go.
                                                                  EJU43580
                                                                  Starting the engine on water
                            At very slow speeds, it may be necessary to
                                                                  EWJ01531
                            support your upper-body weight with your el-
                            bows resting on the gunwales, trailing your
                                                                  Do not apply throttle when anyone is at the
                            legs in the water.
                                                                  rear of the watercraft. Turn the engine off
                            Standing
                            After you are comfortable handling the water-  or keep it at idle. Water and debris exiting
                                                                  the jet thrust nozzle can cause severe in-
                            craft from a kneeling position, try standing as
                                                                  jury.
                            the  watercraft gains  speed. The watercraft
                            will become easier to balance as the speed  To start the engine:
                            increases, because jet thrust provides stabil-  (1) Move the  watercraft to an  area  that is
                            ity as well as directional control. When you  free from weeds and debris, and has a
                            are moving slowly, or preparing to stop, you  water depth of at least 60 cm (2 ft) from
                                                                     the bottom of the watercraft.  NOTICE:
                                                                     Never run the engine in water that is
                                                                     less than 60 cm (2 ft) deep from the
                                                                     bottom  of the watercraft, otherwise
                                                                     pebbles or sand could be sucked into

                                                                                                   54

| 54 55 56 57 58 59 60 61 62 63 64 |