Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 35 - LIT-18626-12-89
P. 35

    UF4R10E0.book  Page 30  Tuesday, August 4, 2020  1:32 PM

                                                                      Watercraft operation

                            EJU40002                              (3) “L-MODE” indicator light comes on and
                              Watercraft operation modes
                                                                     the L-MODE is activated.
                            EJU45571
                            L-MODE
                            The L-MODE  is a function  that limits the
                            maximum engine speed  to approximately
                            85% of the maximum engine speed in  the
                            normal mode.

                                                                      1

                                                                   1 “L-MODE” indicator light
                                                                  To deactivate the L-MODE:
                                                                  To deactivate the L-MODE, follow the same
                                   1
                                                                  procedure as for activating the L-MODE.

                              1 Engine stop/“L-MODE” switch
                            TIP:
                            The L-MODE can only be activated when the
                            engine is stopped.
                            Activating and deactivating the L-MODE
                            Activation of the L-MODE will be confirmed
                            by the “L-MODE” indicator light. (See page
                            31 for information on the indicator lights.)
                            To activate the L-MODE:
                            (1) Briefly push the start switch to turn the
                                power on.
                            (2) Push the engine stop/“L-MODE” switch
                                three times.

                                                                                                   30

| 30 31 32 33 34 35 36 37 38 39 40 |