Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 32 - LIT-18626-12-89
P. 32

    UF4R10E0.book  Page 27  Tuesday, August 4, 2020  1:32 PM

                            Control function operation

                            EJU31027                              vent accidental starting or unauthorized op-
                              Watercraft control functions
                                                                  eration by children or others.
                            EJU45552
                            Engine stop/“L-MODE” switch “ ”
                            The engine stop/“L-MODE” switch (red but-
                            ton)  stops the engine when the switch is
                            pushed. You can also activate L-MODE.

                                                                  EJU45560
                                   1                              Start switch “  ”
                                                                  ECJ01361

                                                                  Do not run  the engine for  more than 15
                              1 Engine stop/“L-MODE” switch
                                                                  seconds on land without supplying water,
                            EJU31164
                            Engine shut-off switch “  ”           otherwise the engine could overheat.
                            The  engine shut-off switch  automatically
                                                                  The start switch (green button) starts the en-
                            stops the engine when the clip, on the end of
                                                                  gine when the switch is pushed.
                            the engine shut-off cord (lanyard), is removed
                                                                  Release the start switch as soon as the en-
                            from the switch, such as if the operator falls
                                                                  gine starts to run. If the engine does not start
                            off the watercraft.
                                                                  in 5 seconds, release the start switch, wait 15
                            Insert the clip  under the engine  shut-off
                                                                  seconds, and then try again. NOTICE: Never
                            switch before starting the engine.
                                                                  push the start switch while the engine is
                                            1         2           running. Do not operate the start switch
                                                                  for  more than 5  seconds, otherwise  the
                                                                  battery will be discharged and the engine

                                                 3

                              1 Clip
                              2 Engine shut-off switch
                              3 Engine shut-off cord (lanyard)
                            When the engine is not running, remove the
                            clip from the engine shut-off switch to pre-

                            27

| 27 28 29 30 31 32 33 34 35 36 37 |