Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 41 - LIT-18626-12-89
P. 41

    UF4R10E0.book  Page 36  Tuesday, August 4, 2020  1:32 PM

                                                                     Equipment operation

                            To install the storage pouch:         To access the fire extinguisher holder:
                            (1) Bend the owner’s/operator’s manual  (1) Lift the steering pole and support it with
                                slightly to insert it into the storage pouch,  the lock pin.
                                and then add any other small items. Fold
                                the pouch, and then close the zipper.

                                                                                            1

                                                                   1 Steering pole

                            (2) Install the  storage  pouch on the hood
                                and secure it with the bands.                  1
                            (3) Securely install the  hood in its original
                                position.
                            EJU41006
                            Fire extinguisher holder
                            The fire extinguisher holder is located on the
                            hood.

                                                                   1 Lock pin
                                                                  (2) Grasp the tab, and then pull it up.
                                                                                2    3
                                                                                            1

                                                                   1 Band
                                                                   2 Fire extinguisher holder cover
                                                                   3 Tab
                                                                  (3) Remove the fire extinguisher holder cov-
                                                                     er.

                                                                                                   36

| 36 37 38 39 40 41 42 43 44 45 46 |