Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 84 - LIT-18626-12-89
P. 84

    UF4R10E0.book  Page 79  Tuesday, August 4, 2020  1:32 PM

                            Trouble recovery

                                ler, jet pump housing, and jet thrust noz-  (3) Connect the other end of the negative (–)
                                zle.                                 jumper cable to an engine hanger.
                                If debris is difficult to remove, consult a
                                Yamaha dealer.                      2                      3
                            EJU34642
                            Jumping the battery                                                4
                            If the watercraft battery has run down, the en-  1
                            gine can be started using a 12-volt booster
                            battery and jumper cables.
                            EJU34664
                            Connecting the jumper cables
                            EWJ01251

                            To avoid  battery  explosion and serious  1 Positive (+) jumper cable
                            damage to the electrical system:       2 Booster battery
                             Do not reverse the polarity of the jumper  3 Negative (–) jumper cable
                                                                   4 Engine hanger
                              cables when connecting to the batter-
                              ies.                                (4) Start the engine, and then disconnect the
                             Do not connect the negative (–) jumper  jumper cables by reversing  the  steps
                              cable to the negative (–) terminal of the  above. (See page 27 for information on
                              watercraft battery.                    starting the engine.)
                             Do not touch the positive (+) jumper ca-  EJU34706
                                                                  Towing the watercraft
                              ble to the negative (–) jumper cable.
                                                                  EWJ00812
                            (1) Connect the positive (+) jumper cable to
                                the positive (+) battery terminals of both   The  operator of  the towing boat  must
                                batteries.                         keep  speed to a minimum  and avoid
                            (2) Connect one  end of the negative  (–)  traffic or obstacles  which could be  a
                                jumper cable to the negative (–) battery  hazard  to the  operator on the  water-
                                terminal of the booster battery.   craft.
                                                                   The towline should be long enough so
                                                                   that the watercraft will not collide with
                                                                   the towing boat when slowing down.
                                                                  If the watercraft becomes inoperative in the
                                                                  water, it can be towed to shore.
                                                                  To tow the watercraft:
                                                                  Use a towline that is three times the com-
                                                                  bined length of the towing boat and the wa-
                                                                  tercraft.

                            79

| 79 80 81 82 83 84 85 86 87 88 89 |