Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 53 - LIT-18626-12-89
P. 53

    UF4R10E0.book  Page 48  Tuesday, August 4, 2020  1:32 PM

                                                                    Pre-operation checks

                            EJU41561                              the watercraft if the battery does not have
                            Engine oil level check
                            Make sure that the engine oil level is between  sufficient power to start the engine or if it
                                                                  shows any other signs of decreased pow-
                            the minimum and maximum level marks on
                                                                  er. Loss of battery power may leave you
                            the dipstick attached to the oil tank filler cap.
                            (See page 39 for information on checking the  stranded. [EWJ01241]
                            engine oil level.)
                                                                                                  1
                                                                                                 2
                                                   1

                                                                   1 Positive (+) battery terminal: Red lead
                                                                   2 Negative (–) battery terminal: Black lead
                              1 Oil tank filler cap/Dipstick
                                                                  Make sure that the battery is securely held in
                                                                  place.
                                                                  EJU32614
                                                                  Steering system checks
                                                                  Turn the handlebars to the right and left sev-
                                                                  eral times  to  make sure that operation is
                                                                  smooth and unrestricted throughout the
                                                                  whole range, and that the free play is not ex-
                                    1    2      3                 cessive.

                              1 Dipstick
                              2 Maximum level mark
                              3 Minimum level mark
                            EJU32456
                            Bilge water check
                            Make sure that no bilge water has collected in
                            the engine compartment. If bilge water has
                            collected in the engine compartment, drain it.
                            (See page 41 for information on draining the
                            bilge water.)                         Turn the handlebars as far as possible to the
                            EJU32486                              right and left to make sure that the jet thrust
                            Battery checks                        nozzle moves as the handlebars are turned,
                            Make sure that the battery terminals are not
                                                                  and that there is no difference between the
                            damaged and that the battery leads are con-
                            nected properly. WARNING! Never operate

                                                                                                   48

| 48 49 50 51 52 53 54 55 56 57 58 |